BR2_aarch64=y
BR2_cortex_a53=y
BR2_ARM_FPU_VFPV4=y

BR2_TOOLCHAIN_BUILDROOT_CXX=y

BR2_SYSTEM_DHCP="eth0"

# Linux headers same as kernel, a 4.14 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_14=y

BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_TARBALL=y
BR2_LINUX_KERNEL_CUSTOM_TARBALL_LOCATION="$(call github,raspberrypi,linux,c117a8bccf37bfba323065b566cf999ed4629a4a)/linux-c117a8bccf37bfba323065b566cf999ed4629a4a.tar.gz"
BR2_LINUX_KERNEL_DEFCONFIG="bcmrpi3"

# Build the DTB from the kernel sources
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="broadcom/bcm2710-rpi-3-b broadcom/bcm2837-rpi-3-b"

BR2_PACKAGE_RPI_FIRMWARE=y
# BR2_PACKAGE_RPI_FIRMWARE_INSTALL_DTB_OVERLAYS is not set

# Required tools to create the SD image
BR2_PACKAGE_HOST_DOSFSTOOLS=y
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_MTOOLS=y

# Filesystem / image
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
BR2_TARGET_ROOTFS_EXT2_SIZE="120M"
# BR2_TARGET_ROOTFS_TAR is not set
BR2_ROOTFS_POST_BUILD_SCRIPT="board/raspberrypi3-64/post-build.sh"
BR2_ROOTFS_POST_IMAGE_SCRIPT="board/raspberrypi3-64/post-image.sh"
BR2_ROOTFS_POST_SCRIPT_ARGS="--aarch64"
